**Procedure for updating software with Windows XP.**

For now we have no solution with Windows 7.

**Prepare an SD card first.**

1. First Prepare a SD card.

1.1 Format a SD card with VFAT (FAT32)

1.2 Unpack the Zip file to the SD card.

Now is the SD card ready.

**Please see below.**





´

1. Make sure the TT-3606E is configured to boot from floppy as the first boot device in the BIOS, insert the SD Card and reboot. Follow the normal install procedure on the screen.